{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Zestawienia ALL","Katalog"],"not_rendered":{"external_links":1,"defined_names":24},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Zestawienia ALL","index":0,"n_rows":1639,"n_cols":24,"rows_kept":1639,"merged":[[269,18,269,20],[285,14,285,16],[285,19,285,20],[286,14,286,16],[286,19,286,20],[287,14,287,16],[287,19,287,20],[288,14,288,16],[288,19,288,20],[289,19,289,20],[290,19,290,20],[291,19,291,20],[292,19,292,20],[293,19,293,20],[294,19,294,20],[295,19,295,20],[296,19,296,20],[298,19,298,20],[299,19,299,20],[301,14,301,20],[302,14,302,20],[303,14,303,20],[304,14,304,20],[305,14,305,20],[306,14,306,20],[307,14,307,20],[308,14,308,20],[309,14,309,20],[310,14,310,20],[345,18,345,20],[361,14,361,16],[361,19,361,20],[362,14,362,16],[362,19,362,20],[363,14,363,16],[363,19,363,20],[364,14,364,16],[364,19,364,20],[365,19,365,20],[366,19,366,20],[367,19,367,20],[368,19,368,20],[369,19,369,20],[370,19,370,20],[371,19,371,20],[372,19,372,20],[374,19,374,20],[375,19,375,20],[377,14,377,20],[378,14,378,20],[379,14,379,20],[380,14,380,20],[381,14,381,20],[382,14,382,20],[383,14,383,20],[384,14,384,20],[385,14,385,20],[386,14,386,20],[387,19,387,20],[388,19,388,20]],"flags":["formulas_cached_only"]}
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":4,"d":"kvs=4.0"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},{"v":71,"d":"liczba osób            71"},{"v":65,"d":"65 dm3/os d"},{"v":4.615,"d":"4.6 m3/d"},{"v":3.2938883581653906,"d":"Nh=3.29"},{"v":0.2563888888888889,"d":"Gsr=0.3 m3/h"},{"v":18,"d":"18.0 h"},{"v":0.844516376274071,"d":"Gmx=0.8 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.111290940685177,"d":"Vzs2.5= 2.1m3"},{"v":200,"d":"200dm3"},{"v":0.09472877287821546,"d":"fi=0.09"},{"v":0.6136473638189925,"d":"beta=0.61"},null,{"v":47.573484178576805,"d":"Qmx=47.6kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_05","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":43.79001473080231,"d":"Qrd=43.8kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":4,"d":"kvs=4.0"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},{"v":98,"d":"liczba osób            98"},{"v":65,"d":"65 dm3/os d"},{"v":6.37,"d":"6.4 m3/d"},{"v":3.0447858305754947,"d":"Nh=3.04"},{"v":0.3538888888888889,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.0775158744869946,"d":"Gmx=1.1 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.6937896862174866,"d":"Vzs2.5= 2.7m3"},{"v":300,"d":"300dm3"},{"v":0.1113672687719167,"d":"fi=0.11"},{"v":0.6120457897582139,"d":"beta=0.61"},null,{"v":60.69886368957349,"d":"Qmx=60.7kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_06","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":55.72572594646677,"d":"Qrd=55.7kW"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},null,"407 all",null,{"v":244,"d":"liczba osób            244"},{"v":65,"d":"65 dm3/os d"},{"v":15.86,"d":"15.9 m3/d"},{"v":2.4372091208328976,"d":"Nh=2.44"},{"v":0.8811111111111111,"d":"Gsr=0.9 m3/h"},{"v":18,"d":"18.0 h"},{"v":2.1474520364672087,"d":"Gmx=2.1 m3/h"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":5.368630091168022,"d":"Vzs2.5= 5.4m3"},{"v":720,"d":"720dm3"},{"v":0.1341124249153388,"d":"fi=0.13"},{"v":0.6431428327359495,"d":"beta=0.64"},null,{"v":120.97074532983447,"d":"Qmx=121.0kW"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_12","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":116.70220174441332,"d":"Qrd=116.7kW"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},null,"407 all",null,{"v":163,"d":"liczba osób            163"},{"v":65,"d":"65 dm3/os d"},{"v":10.595,"d":"10.6 m3/d"},{"v":2.6893178650768768,"d":"Nh=2.69"},{"v":0.5886111111111112,"d":"Gsr=0.6 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.5829623766938619,"d":"Gmx=1.6 m3/h"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.9574059417346548,"d":"Vzs2.5= 4.0m3"},{"v":400,"d":"400dm3"},{"v":0.1010763125868931,"d":"fi=0.10"},{"v":0.6458138411795127,"d":"beta=0.65"},null,{"v":89.17178837333567,"d":"Qmx=89.2kW"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_13","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":86.38256276134578,"d":"Qrd=86.4kW"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},null,221,null,{"v":221,"d":"liczba osób            221"},{"v":65,"d":"65 dm3/os d"},{"v":14.365,"d":"14.4 m3/d"},{"v":2.4968025406269625,"d":"Nh=2.50"},{"v":0.7980555555555555,"d":"Gsr=0.8 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.992587138672573,"d":"Gmx=2.0 m3/h"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.981467846681433,"d":"Vzs2.5= 5.0m3"},{"v":720,"d":"720dm3"},{"v":0.1445357115934516,"d":"fi=0.14"},{"v":0.6303641332704164,"d":"beta=0.63"},null,{"v":112.24686149284531,"d":"Qmx=112.2kW"}]
["NO1",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_15","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":106.13459333589287,"d":"Qrd=106.1kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},null,"?",null,{"v":150,"d":"liczba osób            150"},{"v":65,"d":"65 dm3/os d"},{"v":9.75,"d":"9.8 m3/d"},{"v":2.7444141202581362,"d":"Nh=2.74"},{"v":0.5416666666666666,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.486557648473157,"d":"Gmx=1.5 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.716394121182893,"d":"Vzs2.5= 3.7m3"},{"v":600,"d":"600dm3"},{"v":0.1614468165741866,"d":"fi=0.16"},{"v":0.5970906741674933,"d":"beta=0.60"},null,{"v":83.741095799934,"d":"Qmx=83.7kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_16","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":75.00154102006086,"d":"Qrd=75.0kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},null,"?",null,{"v":210,"d":"liczba osób            210"},{"v":65,"d":"65 dm3/os d"},{"v":13.65,"d":"13.7 m3/d"},{"v":2.528100906926098,"d":"Nh=2.53"},{"v":0.7583333333333333,"d":"Gsr=0.8 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.9171431877522909,"d":"Gmx=1.9 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.792857969380727,"d":"Vzs2.5= 4.8m3"},{"v":700,"d":"700dm3"},{"v":0.14605064545454183,"d":"fi=0.15"},{"v":0.6263340721402844,"d":"beta=0.63"},null,{"v":107.99693608428156,"d":"Qmx=108.0kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_17","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":101.46324113451313,"d":"Qrd=101.5kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},null,"302 aaa",null,{"v":151,"d":"liczba osób            151"},{"v":65,"d":"65 dm3/os d"},{"v":9.815,"d":"9.8 m3/d"},{"v":2.739968293217676,"d":"Nh=2.74"},{"v":0.5452777777777778,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.494043822107305,"d":"Gmx=1.5 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.735109555268262,"d":"Vzs2.5= 3.7m3"},{"v":600,"d":"600dm3"},{"v":0.16063785844078327,"d":"fi=0.16"},{"v":0.5979706372000859,"d":"beta=0.60"},null,{"v":84.16280859668696,"d":"Qmx=84.2kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_18","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":75.49033242766465,"d":"Qrd=75.5kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},null,"302 all",null,{"v":151,"d":"liczba osób            151"},{"v":65,"d":"65 dm3/os d"},{"v":9.815,"d":"9.8 m3/d"},{"v":2.739968293217676,"d":"Nh=2.74"},{"v":0.5452777777777778,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.494043822107305,"d":"Gmx=1.5 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.735109555268262,"d":"Vzs2.5= 3.7m3"},{"v":600,"d":"600dm3"},{"v":0.16063785844078327,"d":"fi=0.16"},{"v":0.5979706372000859,"d":"beta=0.60"},null,{"v":84.16280859668696,"d":"Qmx=84.2kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_19","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":75.49033242766465,"d":"Qrd=75.5kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},null,"436 all",null,{"v":150,"d":"liczba osób            150"},{"v":65,"d":"65 dm3/os d"},{"v":9.75,"d":"9.8 m3/d"},{"v":2.7444141202581362,"d":"Nh=2.74"},{"v":0.5416666666666666,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.486557648473157,"d":"Gmx=1.5 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.716394121182893,"d":"Vzs2.5= 3.7m3"},{"v":600,"d":"600dm3"},{"v":0.1614468165741866,"d":"fi=0.16"},{"v":0.5970906741674933,"d":"beta=0.60"},null,{"v":83.741095799934,"d":"Qmx=83.7kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_20","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":75.00154102006086,"d":"Qrd=75.0kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},null,"436 all",null,{"v":150,"d":"liczba osób            150"},{"v":65,"d":"65 dm3/os d"},{"v":9.75,"d":"9.8 m3/d"},{"v":2.7444141202581362,"d":"Nh=2.74"},{"v":0.5416666666666666,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.486557648473157,"d":"Gmx=1.5 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.716394121182893,"d":"Vzs2.5= 3.7m3"},{"v":600,"d":"600dm3"},{"v":0.1614468165741866,"d":"fi=0.16"},{"v":0.5970906741674933,"d":"beta=0.60"},null,{"v":83.741095799934,"d":"Qmx=83.7kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_21","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":75.00154102006086,"d":"Qrd=75.0kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},null,"436 all",null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":500,"d":"500dm3"},{"v":0.14569374364994583,"d":"fi=0.15"},{"v":0.6015870838452682,"d":"beta=0.60"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"}]
["NO2",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_22","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":69.78076706151592,"d":"Qrd=69.8kW"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},null,150,null,{"v":150,"d":"liczba osób            150"},{"v":65,"d":"65 dm3/os d"},{"v":9.75,"d":"9.8 m3/d"},{"v":2.7444141202581362,"d":"Nh=2.74"},{"v":0.5416666666666666,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.486557648473157,"d":"Gmx=1.5 m3/h"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.716394121182893,"d":"Vzs2.5= 3.7m3"},{"v":400,"d":"400dm3"},{"v":0.10763121104945776,"d":"fi=0.11"},{"v":0.6359303259046551,"d":"beta=0.64"},null,{"v":83.741095799934,"d":"Qmx=83.7kW"}]
["NO2",null,"mCW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_23","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":79.88025351549747,"d":"Qrd=79.9kW"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":2.5,"d":"kvs=2.5"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},{"$nulls":3},"lato",{"$error":"#VALUE!"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},null,111,null,{"v":111,"d":"liczba osób            111"},{"v":65,"d":"65 dm3/os d"},{"v":7.215,"d":"7.2 m3/d"},{"v":2.95363690324998,"d":"Nh=2.95"},{"v":0.4008333333333333,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.1839161253860337,"d":"Gmx=1.2 m3/h"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.9597903134650845,"d":"Vzs2.5= 3.0m3"},{"v":400,"d":"400dm3"},{"v":0.13514470879246585,"d":"fi=0.14"},{"v":0.5989610943959024,"d":"beta=0.60"},null,{"v":66.69262626771838,"d":"Qmx=66.7kW"}]
["NO1",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO_24","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"dod%=50"},{"v":59.91943262617427,"d":"Qrd=59.9kW"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CT/     inst CT",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CT",{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",12,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",null,null,"lato",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"40 mieszkania",null,{"v":140,"d":"liczba osób            140"},{"v":65,"d":"65 dm3/os d"},{"v":9.1,"d":"9.1 m3/d"},{"v":2.7910053671725255,"d":"Nh=2.79"},{"v":0.5055555555555555,"d":"Gsr=0.5 m3/h"},null,{"v":1.4110082689594434,"d":"Gmx=1.4 m3/h"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},null,"160 os wg proj",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.527520672398609,"d":"Vzs2.5= 3.5m3"},{"v":400,"d":"400dm3"},{"v":0.11339409096304798,"d":"fi=0.11"},{"v":0.6276221658619892,"d":"beta=0.63"},null,{"v":79.48523136441648,"d":"Qmx=79.5kW"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":20,"d":"dod%=20"},{"v":59.86403167557165,"d":"Qrd=59.9kW"}]
["NO3",null,"CO+CW+CT","2011 Wykonane",null,"obliczenia","POZ",null,"NO-25","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",15,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",null,null,"lato",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"43 mieszkania",null,{"v":150.5,"d":"liczba osób            151"},{"v":65,"d":"65 dm3/os d"},{"v":9.7825,"d":"9.8 m3/d"},{"v":2.742186613201803,"d":"Nh=2.74"},{"v":0.5434722222222222,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.4903022524248133,"d":"Gmx=1.5 m3/h"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},null,"172 os wg proj",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.7257556310620332,"d":"Vzs2.5= 3.7m3"},{"v":500,"d":"500dm3"},{"v":0.13420096472013493,"d":"fi=0.13"},{"v":0.6154643798242214,"d":"beta=0.62"},null,{"v":83.95203766187291,"d":"Qmx=84.0kW"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":25,"d":"dod%=25"},{"v":64.58686099318037,"d":"Qrd=64.6kW"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-32","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",15,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",null,null,"lato",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"52 mieszkania",null,{"v":182,"d":"liczba osób            182"},{"v":65,"d":"65 dm3/os d"},{"v":11.83,"d":"11.8 m3/d"},{"v":2.6179327956586604,"d":"Nh=2.62"},{"v":0.6572222222222223,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7205636095912198,"d":"Gmx=1.7 m3/h"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},null,"208 os wg proj",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.301409023978049,"d":"Vzs2.5= 4.3m3"},{"v":500,"d":"500dm3"},{"v":0.11624097992373383,"d":"fi=0.12"},{"v":0.6391374612000488,"d":"beta=0.64"},null,{"v":96.9231716029614,"d":"Qmx=96.9kW"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":25,"d":"dod%=25"},{"v":77.43403728721677,"d":"Qrd=77.4kW"}]
["NO3",null,"CO+CW","2011 Wykonane",null,"obliczenia","POZ",null,"NO-33","OK",{"$error":"#N/A"}]
["NO3",null,"CO",2011,null,"obliczenia","A+Q",null,"NO-34","OK",{"$error":"#N/A"},null,"Ciśnienie dyspozycyjne sieć:",null,null,{"v":50,"d":"50.0 kPa"},null,"Opory węzła:",{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.7000000000000002,"d":"p1=1.7"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-34","OK",{"$error":"#N/A"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},null,"Opory wymiennika CO str. pierw.",null,null,{"v":2,"d":"2.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},null,"Zawór reg CO MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.7000000000000002,"d":"p1=1.7"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-35","OK",{"$error":"#N/A"}]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 7","OK",{"$error":"#N/A"},{"$nulls":4},"Bluszcza 7"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 7","OK",{"$error":"#N/A"},null," Moc [kW]",null,"   Obieg","            Sieć: temperatura [C], przepływ [m3/h], średnica [mm]",{"$nulls":3}," Instalacja: temp [C], przepływ m3/h], średn [mm]"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,{"v":80,"d":"80.0"},null,"moduł CO",{"v":130,"d":"130 / "},78,{"v":1.3834313924436197,"d":"1.4 m3/h"},"Dn32",{"v":90,"d":"90 / "},70,{"v":3.536716097394492,"d":"3.5 m3/h"},"Dn50"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,{"v":80,"d":"80.0"},null,"RAZEM przyłącze MAX",{"v":130,"d":"130 / "},78,{"v":1.3834313924436197,"d":"1.4 m3/h"},"Dn32","-","-","-","-"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,"Ciśnienie dyspozycyjne sieć:",null,null,{"v":300,"d":"300.0 kPa"},null,"Opory węzła:",{"v":53.33722139372089,"d":"53.3 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,"Opory wymiennika CO str. pierw.",null,null,{"v":2,"d":"2.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"v":4.822077141845535,"d":"4.8 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,"Zawór reg CO MAX",null,null,{"v":31.515144251875356,"d":"31.5 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"v":0.47782106019076787,"d":"0.48 m/s"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"v":4.822077141845535,"d":"5 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"v":0.47782106019076787,"d":"0.48 m/s"},null,{"v":50,"d":"Dn50"},{"v":0.5003429770782316,"d":"0.50 m/s"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"v":31.515144251875356,"d":"32 kPa"},{"v":1,"d":"wsp.b=1.0"},null,"NG80/1,7"]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",12,{"v":0.96,"d":"1.0m3"},{"v":1.7000000000000002,"d":"p1=1.7"},{"v":4,"d":"p2=4.0"},{"v":0.03564493488605631,"d":"0.0356"},{"v":34.20887174936687,"d":"34 dm3"},{"v":74.36711249862364,"d":"74 dm3"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 7","OK",{"$error":"#N/A"}]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZR-bezp_d","Bluszcza 7","OK",{"$error":"#N/A"},null,1,null,"Zawór reg., stab. różnicy ciśnień z ogr. przepływu","typ AVPB",{"v":6.3,"d":"kvs=6.3"},"Dn20","zakres 0,3-2,0 bar",null,"PN25, Tmax130C","Danfoss\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZR-bezp_d","Bluszcza 7","OK",{"$error":"#N/A"},null,"1a",null,"Zawór impulsowy, końc. redukcyjna, końc. do przewodu impulsowego","typ ZWZ-11",{"$nulls":4},"PN16, Tmax130C","Polna\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","F-Sieć","Bluszcza 7","OK",{"$error":"#N/A"},null,2,null,"Filtroodmulnik magnet., izolacja","typ FM-Aulin",null,"Dn32",null,null,"PN16, Tmax130C","Aulin\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Sieć","Bluszcza 7","OK",{"$error":"#N/A"},null,3,null,"Zawór kulowy,kołn.",null,null,"Dn32",null,null,"PN16, Tmax130C","Naval\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Sieć","Bluszcza 7","OK",{"$error":"#N/A"},null,4,null,"Zawór kulowy, spaw.-kołn., odwodn./odp.",null,null,"Dn15",null,null,"PN16, Tmax130C","Naval\nlub równoważny",4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},5,null,"Zawór kulowy, spaw.-kołn.",null,null,"Dn15",null,null,"PN16, Tmax130C","Naval\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 7","OK",{"$error":"#N/A"},null,6,null,"Zawór kulowy, spaw.-kołn.",null,null,"Dn25",null,null,"PN16, Tmax130C","Naval\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},7,null,"Wymiennik lut. z izol.\nTyp XB12L-1-36","Q=80,0 [kW]","Ts=130/78","Ti=90/70","dps/i=3/12kPa","+15% mocy","PN25, Tmax130C","Sondex\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},8,null,"Zawór reg. przelotowy/ siłownik","typ VM2",{"v":6.3,"d":"kvs=6.3"},"Dn20","typ AMV23","U=230V","PN25, Tmax130C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},"8a",null,"Termostat","St-1","Zakres 30-120","dł .200[mm]",null,null,"PN6, Tmax100C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},"8b",null,"Zawór balansowy / ręczna regulacja,\nkołn.","typ MSV-F2",null,"Dn25",null,null,"PN25, Tmax150C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},9,null,"Licznik ciepła CO czujniki, zasil. 230V","typ UH50","Qp= 1,5 m3/h","Dn25","montaż powrót",null,"PN16, Tmax130C","Landys+Gyr\nlub równoważny","1"]
["NO3",null,"CO",2011,null,"ZEST","POZ","Wodomierz","Bluszcza 7","OK",{"$error":"#N/A"},null,10,null,"Wodomierz w.gorąca, z impls. 10 dm3/imp. z półśr.","typ JS90-2,5NK",null,"Dn15",null,null,"PN16, Tmax130C","Powogaz\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","F-Sieć","Bluszcza 7","OK",{"$error":"#N/A"},null,11,null,"Filtr siatkowy, kołnierz.",null,null,"Dn15",null,null,"PN16, Tmax130C","Zetkama\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},12,null,"Zawór napełniania instalacji, z manometrem","zawór typ 2128",null,"Dn15",null,null,"PN16, Tmax130C","SYR\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZZ","Bluszcza 7","OK",{"$error":"#N/A"},null,13,null,"Zawór zwrotny, płytkowy","typ 812",null,"Dn15",null,null,"PN16, Tmax130C","Socla\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Sieć","Bluszcza 7","OK",{"$error":"#N/A"},null,14,null,"Zawór kulowy, spaw.",null,null,"Dn15",null,null,"PN16, Tmax130C","DZT\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 7","OK",{"$error":"#N/A"},null,15,null,"Zawór kulowy, gwint.",null,null,"Dn15",null,null,"PN6, Tmax100C","Valvex\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","Pompa","Bluszcza 7","OK",{"$error":"#N/A"},null,16,null,"Pompa obiegowa","typ Magna 3 32-120\n",{"v":3.536716097394492,"d":"V= 3.5 [m3/h]"},{"v":7,"d":"H= 7.0 [m]"},"~230/240V; 29-1301W;0,3-5,68A",null,null,"Grundfos\nlub równoważny",2,"Zwykłe czy kołnierzowe, sprawdzić cene która tańsza"]
["NO3",null,"CO",2011,null,"ZEST","POZ","Z_bezpiecz","Bluszcza 7","OK",{"$error":"#N/A"},null,17,null,"Zawór bezp.","typ 1915",null,"Dn25","p=4,0 bar",null,"PN6, Tmax100C","Syr\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","NW","Bluszcza 7","OK",{"$error":"#N/A"},null,18,null,"Przep. naczynie wzb., szybkozłączka SU1”","typ NG80/1,7",{"$nulls":4},"PN6, Tmax50C","Reflex\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","F-Inst_CO","Bluszcza 7","OK",{"$error":"#N/A"},null,19,null,"Filtr siatkowy z wkładką magnetyczną , kołnierz.",null,null,"Dn50",null,null,"PN6, Tmax100C","Zetkama\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 7","OK",{"$error":"#N/A"},null,20,null,"Zawór kulowy, kołnierz.",null,null,"Dn50",null,null,"PN6, Tmax100C","Naval\nlub równoważny",6]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},21,null,"Zawór zwrotny, międzykołnierzowy",null,null,"Dn50",{"$nulls":3},"socla",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 7","OK",{"$error":"#N/A"},null,22,null,"Zawór kulowy, gwint., odwodnienia/ odp.",null,null,"Dn15  ",null,null,"PN6, Tmax100C","Valvex\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,23,null,"Sterownik węzła","typ ECL 310",{"$nulls":5},"Danfoss\nlub równoważny","wg \nAKPiA"]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,"te",null,"Czujnik temp. zewn.","typ ESMT","Pt1000",{"$nulls":4},"Danfoss\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,"t",null,"Czujnik temp. zanurz.","typ ESMU","Pt1000",{"$nulls":4},"Danfoss\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,"PI",null,"Manometr z kurkiem i rurką syfonową","0-1,6MPa",{"$nulls":4},"PN16, Tmax130C","Wika\nlub równoważny",4]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,"PI",null,"Manometr z kurkiem i rurką syfonową","0-0,6MPa",{"$nulls":4},"PN6, Tmax100C","Wika\nlub równoważny",3]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,"TI ",null,"Termometr techniczny prosty","0-150C",{"$nulls":4},"PN16, Tmax130C","Wika\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},"TI ",null,"Termometr techniczny prosty","0-100C",{"$nulls":4},"PN6, Tmax100C","Wika\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 7","OK",{"$error":"#N/A"},null,"PidP",null,"Prezostat różnicy ciśnień","Typ RT263AL","0,1-1,0 bar",{"$nulls":3},"PN6, Tmax100C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":6},"Rozdzielacze c.o. "]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},24,null,"Rura stalowa bez szwu DN80 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"1,4 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},25,null,"Rura stalowa bez szwu DN50 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"1 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},26,null,"Rura stalowa bez szwu DN40 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"2 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},27,null,"Rura stalowa bez szwu DN25 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"1 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},28,null,"Dennice stalowe Dn80",{"$nulls":4},"PN6, Tmax100C",null,null,4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},29,null,"Zawór kulowy, gwint.",null,null,"Dn40",null,"PN6, Tmax100C",null,"Valvex\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},30,null,"Zawór balansowy / ręczna regulacja, gwint.","typ MSV-B",null,"Dn40",null,"PN6, Tmax100C",null,"Danfoss\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},31,null,"Zawór kulowy, gwint.",null,null,"Dn25",null,"PN6, Tmax100C",null,"Valvex\nlub równoważny",3]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},32,null,"Zawór balansowy / ręczna regulacja, gwint.","typ MSV-B",null,"Dn25",null,"PN6, Tmax100C",null,"Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},33,null,"Dwuzłączka",null,null,"Dn50",null,"PN6, Tmax100C",null,null,2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},34,null,"Dwuzłączka",null,null,"Dn40",null,"PN6, Tmax100C",null,null,4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},35,null,"Dwuzłączka",null,null,"Dn25",null,"PN6, Tmax100C",null,null,2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},36,null,"Stalowa konstrukcja wsporcza pod rozdzielacz",{"$nulls":7},2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},37,null,"Termometr techniczny prosty","0-100C",{"$nulls":3},"PN6, Tmax100C",null,"Wika\nlub równoważny",5]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},38,null,"Manometr z kurkiem i rurką syfonową","0-0,6MPa",{"$nulls":3},"PN6, Tmax100C",null,"Wika\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":6},"Materiały dodatkowe"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},39,null,"Rura stalowa bez szwu DN32 wraz z izolacją cieplną, PN16",{"$nulls":7},"14mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},40,null,"Rura stalowa bez szwu DN20 wraz z izolacją cieplną, PN16",{"$nulls":7},"2mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},41,null,"Rura stalowa bez szwu DN15 wraz z izolacją cieplną, PN16",{"$nulls":7},"6mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},42,null,"Rura stalowa bez szwu DN50 wraz z izolacją cieplną, PN6",{"$nulls":7},"14mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},43,null,"Rura stalowa bez szwu DN40 wraz z izolacją cieplną, PN6",{"$nulls":7},"16mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},44,null,"Rura stalowa bez szwu DN25 wraz z izolacją cieplną, PN6",{"$nulls":7},"12mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},45,null,"Rura stalowa bez szwu DN20, PN6",{"$nulls":7},"8mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},46,null,"Rura stalowa bez szwu DN15, PN6",{"$nulls":7},"4mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},47,null,"Stalowa konstrukcja wsporcza  węzła cieplnego",{"$nulls":7},1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 7",{"$nulls":3},48,null,"Kratka wentylacyjna",{"$nulls":7},2]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 13","OK",{"$error":"#N/A"},{"$nulls":4},"Bluszcza 13"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 13","OK",{"$error":"#N/A"},null," Moc [kW]",null,"   Obieg","            Sieć: temperatura [C], przepływ [m3/h], średnica [mm]",{"$nulls":3}," Instalacja: temp [C], przepływ m3/h], średn [mm]"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,{"v":360,"d":"360.0"},null,"moduł CO",{"v":130,"d":"130 / "},78,{"v":6.225441265996288,"d":"6.2 m3/h"},"Dn50",{"v":90,"d":"90 / "},70,{"v":15.915222438275213,"d":"15.9 m3/h"},"Dn80"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,{"v":360,"d":"360.0"},null,"RAZEM przyłącze MAX",{"v":130,"d":"130 / "},78,{"v":6.225441265996288,"d":"6.2 m3/h"},"Dn50","-","-","-","-"]
["NO3",null,"CO",2011,null,"ZEST","A+Q",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,"Ciśnienie dyspozycyjne sieć:",null,null,{"v":300,"d":"300.0 kPa"},null,"Opory węzła:"]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,"Opory wymiennika CO str. pierw.",null,null,{"v":2,"d":"2.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"v":24.803916132076456,"d":"24.8 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,"Zawór reg CO MAX",null,null,{"v":38.75611895636946,"d":"38.8 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"v":0.8807197781436229,"d":"0.88 m/s"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"v":24.803916132076456,"d":"25 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":50,"d":"Dn50"},{"v":0.8807197781436229,"d":"0.88 m/s"},null,{"v":80,"d":"Dn80"},{"v":0.8795091393953289,"d":"0.88 m/s"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"v":38.75611895636946,"d":"39 kPa"},{"v":1.1,"d":"wsp.b=1.1"},null,"N500/1,7"]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"v":4.86,"d":"4.9m3"},{"v":1.7000000000000002,"d":"p1=1.7"},{"v":4,"d":"p2=4.0"},{"v":0.03564493488605631,"d":"0.0356"},{"v":173.1824132311698,"d":"173 dm3"},{"v":376.4835070242822,"d":"376 dm3"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"Bluszcza 13","OK",{"$error":"#N/A"}]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZR-bezp_d","Bluszcza 13","OK",{"$error":"#N/A"},null,1,null,"Zawór reg., stab. różnicy ciśnień z ogr. przepływu","typ AVPB",{"v":12.5,"d":"kvs=12.5"},"Dn32","zakres 0,3-2,0 bar",null,"PN25, Tmax130C","Danfoss\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZR-bezp_d","Bluszcza 13","OK",{"$error":"#N/A"},null,"1a",null,"Zawór impulsowy, końc. redukcyjna, końc. do przewodu impulsowego","typ ZWZ-11",{"$nulls":4},"PN16, Tmax130C","Polna\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","F-Sieć","Bluszcza 13","OK",{"$error":"#N/A"},null,2,null,"Filtroodmulnik magnet., izolacja","typ FM-Aulin",null,"Dn50",null,null,"PN16, Tmax130C","Aulin\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Sieć","Bluszcza 13","OK",{"$error":"#N/A"},null,3,null,"Zawór kulowy,kołn.",null,null,"Dn50",null,null,"PN16, Tmax130C","Naval\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Sieć","Bluszcza 13","OK",{"$error":"#N/A"},null,4,null,"Zawór kulowy, spaw.-kołn., odwodn./odp.",null,null,"Dn15",null,null,"PN16, Tmax130C","Naval\nlub równoważny",4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},5,null,"Zawór kulowy, spaw.-kołn.",null,null,"Dn15",null,null,"PN16, Tmax130C","Naval\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 13","OK",{"$error":"#N/A"},null,6,null,"Zawór kulowy, spaw.-kołn.",null,null,"Dn25",null,null,"PN16, Tmax130C","Naval\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},7,null,"Wymiennik lut. z izol.\nTyp XB52M-1","Q=360,0 [kW]","Ts=130/78","Ti=90/70","dps/i=3/15kPa","+15% mocy","PN25, Tmax130C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},8,null,"Zawór reg. przelotowy/ siłownik","typ VM2",{"v":10,"d":"kvs=10.0"},"Dn32","typ AMV23","U=230V","PN25, Tmax130C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},"8a",null,"Termostat","St-1","Zakres 30-120","dł .200[mm]",null,null,"PN6, Tmax100C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},"8b",null,"Zawór balansowy / ręczna regulacja,\nkołn.","typ MSV-F2",null,"Dn40",null,null,"PN25, Tmax150C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},9,null,"Licznik ciepła CO czujniki, zasil. 230V","typ UH50","Qp= 10 m3/h","Dn50","montaż powrót",null,"PN16, Tmax130C","Landys+Gyr\nlub równoważny","1"]
["NO3",null,"CO",2011,null,"ZEST","POZ","Wodomierz","Bluszcza 13","OK",{"$error":"#N/A"},null,10,null,"Wodomierz w.gorąca, z impls. 10 dm3/imp. z półśr.","typ JS90-2,5NK",null,"Dn20",null,null,"PN16, Tmax130C","Powogaz\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","F-Sieć","Bluszcza 13","OK",{"$error":"#N/A"},null,11,null,"Filtr siatkowy, kołnierz.",null,null,"Dn20",null,null,"PN16, Tmax130C","Zetkama\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},12,null,"Zawór napełniania instalacji, z manometrem","zawór typ 2128",null,"Dn20",null,null,"PN16, Tmax130C","SYR\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZZ","Bluszcza 13","OK",{"$error":"#N/A"},null,13,null,"Zawór zwrotny, płytkowy","typ 812",null,"Dn20",null,null,"PN16, Tmax130C","Socla\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Sieć","Bluszcza 13","OK",{"$error":"#N/A"},null,14,null,"Zawór kulowy, spaw.",null,null,"Dn20",null,null,"PN16, Tmax130C","DZT\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 13","OK",{"$error":"#N/A"},null,15,null,"Zawór kulowy, gwint.",null,null,"Dn20",null,null,"PN6, Tmax100C","Valvex\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","Pompa","Bluszcza 13","OK",{"$error":"#N/A"},null,16,null,"Pompa obiegowa","typ Magna 3 65-150F\n",{"v":15.915222438275213,"d":"V= 15.9 [m3/h]"},{"v":10,"d":"H= 10.0 [m]"},"~230/240V; 29-1301W;0,3-5,68A",null,null,"Grundfos\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","Z_bezpiecz","Bluszcza 13","OK",{"$error":"#N/A"},null,17,null,"Zawór bezp.","typ 1915",null,"Dn25","p=5,0 bar",null,"PN6, Tmax100C","Syr\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","NW","Bluszcza 13","OK",{"$error":"#N/A"},null,18,null,"Przep. naczynie wzb., szybkozłączka SU1”","typ N500/1,7",{"$nulls":4},"PN6, Tmax50C","Reflex\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","F-Inst_CO","Bluszcza 13","OK",{"$error":"#N/A"},null,19,null,"Filtr siatkowy z wkładką magnetyczną , kołnierz.",null,null,"Dn80",null,null,"PN6, Tmax100C","Zetkama\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 13","OK",{"$error":"#N/A"},null,20,null,"Zawór kulowy, kołnierz.",null,null,"Dn80",null,null,"PN6, Tmax100C","Naval\nlub równoważny",6]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},21,null,"Zawór zwrotny, międzykołnierzowy",null,null,"Dn80",{"$nulls":3},"socla",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","ZO-Inst_CO","Bluszcza 13","OK",{"$error":"#N/A"},null,22,null,"Zawór kulowy, gwint., odwodnienia/ odp.",null,null,"Dn15  ",null,null,"PN6, Tmax100C","Valvex\nlub równoważny",2,"2010-01-25"]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,23,null,"Sterownik węzła","typ ECL 310",{"$nulls":5},"Danfoss\nlub równoważny","wg \nAKPiA"]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,"te",null,"Czujnik temp. zewn.","typ ESMT","Pt1000",{"$nulls":4},"Danfoss\nlub równoważny",1]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,"t",null,"Czujnik temp. zanurz.","typ ESMU","Pt1000",{"$nulls":4},"Danfoss\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,"PI",null,"Manometr z kurkiem i rurką syfonową","0-1,6MPa",{"$nulls":4},"PN16, Tmax130C","Wika\nlub równoważny",4]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,"PI",null,"Manometr z kurkiem i rurką syfonową","0-0,6MPa",{"$nulls":4},"PN6, Tmax100C","Wika\nlub równoważny",3]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,"TI ",null,"Termometr techniczny prosty","0-150C",{"$nulls":4},"PN16, Tmax130C","Wika\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},"TI ",null,"Termometr techniczny prosty","0-100C",{"$nulls":4},"PN6, Tmax100C","Wika\nlub równoważny",2]
["NO3",null,"CO",2011,null,"ZEST","POZ","AKPiA","Bluszcza 13","OK",{"$error":"#N/A"},null,"PidP",null,"Prezostat różnicy ciśnień","Typ RT263AL","0,1-1,0 bar",{"$nulls":3},"PN6, Tmax100C","Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":6},"Rozdzielacze c.o. "]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},24,null,"Rura stalowa bez szwu DN125 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"2 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},25,null,"Rura stalowa bez szwu DN80 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"2 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},26,null,"Rura stalowa bez szwu DN50 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"2 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},27,null,"Rura stalowa bez szwu DN25 wraz z izolacją cieplną",{"$nulls":4},"PN6, Tmax100C",null,null,"0,5 mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},28,null,"Dennice stalowe Dn125",{"$nulls":4},"PN6, Tmax100C",null,null,4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},29,null,"Zawór kulowy, kołnierz.",null,null,"Dn80",null,"PN6, Tmax100C",null,"Valvex\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},30,null,"Zawór balansowy / ręczna regulacja, gwint.","typ MSV-F2",null,"Dn80",null,"PN6, Tmax100C",null,"Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},31,null,"Zawór kulowy, gwint.",null,null,"Dn50",null,"PN6, Tmax100C",null,"Valvex\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},32,null,"Zawór balansowy / ręczna regulacja, gwint.","typ MSV-B",null,"Dn50",null,"PN6, Tmax100C",null,"Danfoss\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},33,null,"Zawór kulowy, gwint.",null,null,"Dn25",null,"PN6, Tmax100C",null,"Valvex\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},34,null,"Dwuzłączka",null,null,"Dn80",null,"PN6, Tmax100C",null,null,4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},35,null,"Dwuzłączka",null,null,"Dn50",null,"PN6, Tmax100C",null,null,4]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},36,null,"Stalowa konstrukcja wsporcza pod rozdzielacz",{"$nulls":7},2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},37,null,"Termometr techniczny prosty","0-100C",{"$nulls":3},"PN6, Tmax100C",null,"Wika\nlub równoważny",5]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},38,null,"Manometr z kurkiem i rurką syfonową","0-0,6MPa",{"$nulls":3},"PN6, Tmax100C",null,"Wika\nlub równoważny",2]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":6},"Materiały dodatkowe"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},39,null,"Rura stalowa bez szwu DN50 wraz z izolacją cieplną, PN16",{"$nulls":7},"16mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},40,null,"Rura stalowa bez szwu DN20 wraz z izolacją cieplną, PN16",{"$nulls":7},"2mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},41,null,"Rura stalowa bez szwu DN15 wraz z izolacją cieplną, PN16",{"$nulls":7},"6mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},42,null,"Rura stalowa bez szwu DN80 wraz z izolacją cieplną, PN6",{"$nulls":7},"20mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},43,null,"Rura stalowa bez szwu DN50 wraz z izolacją cieplną, PN6",{"$nulls":7},"30mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},44,null,"Rura stalowa bez szwu DN32 wraz z izolacją cieplną, PN6",{"$nulls":7},"10mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},45,null,"Rura stalowa bez szwu DN20, PN6",{"$nulls":7},"8mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},46,null,"Rura stalowa bez szwu DN15, PN6",{"$nulls":7},"4mb"]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},47,null,"Stalowa konstrukcja wsporcza  węzła cieplnego",{"$nulls":7},1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},48,null,"Kratka wentylacyjna",{"$nulls":7},1]
[{"$nulls":5},"ZEST",null,null,"Bluszcza 13",{"$nulls":3},49,null,"Zawór kulowy, gwint.",null,null,"Dn32",null,"PN6, Tmax100C",null,"Valvex\nlub równoważny",1]
[{"$nulls":5},"ZEST",{"$nulls":6},50,null,"Zawór balansowy / ręczna regulacja, gwint.","typ MSV-B",null,"Dn32",null,"PN6, Tmax100C",null,"Danfoss\nlub równoważny",1]
[{"$nulls":5},"ZEST"]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},null,282.6,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"v":0,"d":"0 kPa"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},null,0.7,null,"sieć  CO/     inst CO",{"v":50,"d":"Dn50"},{"v":0,"d":"0.00 m/s"},null,{"v":65,"d":"Dn65"},{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"Czujnik temp. zanurz.",{"v":10,"d":"kvs=10.0"},"Dn25",null,{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"Manometr z kurkiem i rurką syfonową",{"v":16,"d":"kvs=16.0"},"Dn32",null,{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"Czujnik temp. zewn.",null,null,{"v":65,"d":"Dn65"},{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"Czujnik temp. zanurz.",null,null,{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"Manometr z kurkiem i rurką syfonową",null,null,{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"CT nie ma w bilansie",null,null,{"v":40,"d":"Dn40"},"-"]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},null,197.82000000000002,null,"z.reg CO",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"v":0,"d":"0 kPa"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"}]
["NO5",null,"CO",2011,null,"obliczenia","POZ",null,"NO-36","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"v":-0.00156896015073913,"d":"-0.0016"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":5,"d":"5.0 kPa"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":0,"d":"0.0 kPa"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":16,"d":"kvs=16.0"},"Dn40","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":12.5,"d":"kvs=12.5"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2.5,"d":"p1=2.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"Wałaszek podał",null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},null,"400 os",null,{"v":400,"d":"liczba osób            400"},{"v":6,"d":"6 dm3/os d"},{"v":2.4,"d":"2.4 m3/d"},{"v":3.5,"d":"Nh=3.50"},{"v":0.3,"d":"Gsr=0.3 m3/h"},{"v":8,"d":"8 h"},{"v":1.05,"d":"Gmx=1.1 m3/h"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.625,"d":"Vzs2.5= 2.6m3"},{"v":400,"d":"400dm3"},{"v":0.1523809523809524,"d":"fi=0.15"},{"v":0.5537228661542491,"d":"beta=0.55"},"str cyrk+%",{"v":59.14883333333334,"d":"Qmx=59.1kW"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},"miesiąc",{"v":48,"d":"48.0m3"},null,{"$error":"#REF!"},{"v":20,"d":"dod%=20"},{"v":39.302473827616,"d":"Qrd=39.3kW"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"Obieg kotła CW",{"v":32,"d":"Dn32"},{"$error":"#REF!"},null,null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO5",null,"KG+GAZ",2011,null,"obliczenia","POZ",null,"NO-39","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1,"d":"p1=1.0"},{"v":3,"d":"p2=3.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,"-"]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":4,"d":"4.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":65,"d":"Dn65"},{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":20,"d":"kvs=20.0"},"Dn50","zima",{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":65,"d":"Dn65"},{"$error":"#VALUE!"},null,{"v":100,"d":"Dn100"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":25,"d":"kvs=25.0"},"Dn50","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-40","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":16,"d":"kvs=16.0"},"Dn40","zima",{"$error":"#VALUE!"},"lato","brak"]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CT/     inst CT",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CT",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO1",{"v":16,"d":"kvs=16.0"},"Dn32",null,null,"lato",{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO2",{"v":10,"d":"kvs=10.0"},"Dn25",null,null,"lato",{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO3",{"v":6.3,"d":"kvs=6.3"},"Dn20",null,null,"lato",{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3}," inst CO1",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3}," inst CO2",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3}," inst CO3",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3}," inst CT1",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3}," inst CT2",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3}," inst CT3",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"rozdz./ licznik CO PROK  LC co 1",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"rozdzielacz/ licznik CO SĄD  LC co 2",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"rozdz./ licznik CT PROK  LC ct 3",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO3",null,"CO+CT",2011,null,"obliczenia","POZ",null,"NO-41","OK",{"$error":"#N/A"},{"$nulls":3},"rozdzielacz/ licznik CT SĄD  LC ct 4",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
[{"$nulls":9},"OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,"-"]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":4,"d":"4.0 kPa"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":65,"d":"Dn65"},{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":32,"d":"kvs=32.0"},"zima",{"$error":"#VALUE!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":65,"d":"Dn65"},{"$error":"#VALUE!"},null,{"v":125,"d":"Dn125"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":25,"d":"kvs=25.0"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"liczba skazanych ",{"v":750,"d":"750 os"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"natryski parter/ 1p/ 2p/ 3p/     /cele",{"v":15,"d":"15 szt."},{"v":3,"d":"3 szt."},{"v":3,"d":"3 szt."},{"v":3,"d":"3 szt."},null,{"v":280,"d":"280 szt."}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"kuchnia całodobowa posiłki S+O+K",{"v":1000,"d":"1000 szt."}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":7},"przepływ dławiony  cela",null,{"v":8,"d":"8 dm3/min"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,null,"Natryski"]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},{"v":200,"d":"liczba osób            200"},{"v":45,"d":"45 dm3/os d"},{"v":9,"d":"9.0 m3/d"},{"v":1,"d":"Nh=1.00"},{"v":2.25,"d":"Gsr=2.3 m3/h"},{"v":4,"d":"4 h/dzień"},{"v":2.25,"d":"Gmx=2.3 m3/h"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"Przepływ ciągły","przepływ dławiony natrysk",null,{"v":10,"d":"10 dm3/min"},{"v":15,"d":"15 szt."},{"v":36,"d":"36.0 m3/d"},{"v":2.5,"d":"Gmx=2.5 m3/h"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":9},{"v":140.83055555555558,"d":"Qmx=140.8kW"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,null,"cela"]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},{"v":750,"d":"liczba osób            750"},{"v":6,"d":"6 dm3/os d"},{"v":4.5,"d":"4.5 m3/d"},{"v":1,"d":"Nh=1.00"},{"v":4.5,"d":"Gsr=4.5 m3/h"},{"v":1,"d":"1 h/dzień"},{"v":4.5,"d":"Gmx=4.5 m3/h"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"Przepływ ciągły","przepływ dławiony cela",null,{"v":8,"d":"8 dm3/min"},{"v":280,"d":"280 szt."},{"v":47.040000000000006,"d":"47.0 m3/d"},{"v":9.333333333333334,"d":"Gmx=9.3 m3/h"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"liczba równych sekcji",{"v":4,"d":"4 szt."},null,"czas otwarcia",{"v":0.35,"d":"35.00%"},null,{"v":525.7674074074075,"d":"Qmx=525.8kW"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,288,null,"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"v":0,"d":"0.00 m/s"},null,{"v":40,"d":"Dn40"},{"v":0,"d":"0.00 m/s"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,"238,5 na 288",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"v":0,"d":"0.00 m/s"},{"v":25,"d":"Dn25"},{"v":0,"d":"0.00 m/s"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":10,"d":"kvs=10.0"},{"$nulls":3},"lato",{"v":0,"d":"0 kPa"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},null,238.5,null,{"v":418,"d":"liczba osób            418"},{"v":20,"d":"20 dm3/os d"},{"v":8.36,"d":"8.4 m3/d"},{"v":2.5,"d":"Nh=2.50"},{"v":0.46444444444444444,"d":"Gsr=0.5 m3/h"},null,{"v":1.161111111111111,"d":"Gmx=1.2 m3/h"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.9027777777777777,"d":"Vzs2.5= 2.9m3"},{"v":400,"d":"400dm3"},{"v":0.13779904306220098,"d":"fi=0.14"},{"v":0.6344365218239312,"d":"beta=0.63"},null,{"v":65.40796913580247,"d":"Qmx=65.4kW"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"},{"$nulls":3},{"v":0,"d":"Pojemność cieplna  0"},{"$nulls":3},{"v":0,"d":"czas ład= 0min"},{"v":50,"d":"dod%=50"},{"v":62.24580665712834,"d":"Qrd=62.2kW"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO+CW+KG[istn.]",2011,null,"obliczenia","POZ",null,"NO-42","OK",{"$error":"#N/A"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,"-"]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":4,"d":"4.0 kPa"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"CO",2011,null,"obliczenia","POZ",null,"NO-43","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":5,"d":"5.0 kPa"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":65,"d":"Dn65"},{"$error":"#VALUE!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":16,"d":"kvs=16.0"},"Dn40","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"CO bud 1",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"CO bud 2",{"$nulls":3},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO bud 1",{"v":16,"d":"kvs=16.0"},"Dn32",null,null,"lato",{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO bud 2",{"v":4,"d":"kvs=4.0"},"Dn15",null,null,"lato",{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CT/     inst CT",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CT",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",12,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CW/     inst CW",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",12,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"osadzonych",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,311,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
[null,null,"KG+GAZ",2012,{"$nulls":4},"NO-44","OK",{"$error":"#N/A"},{"$nulls":6},{"$error":"#NUM!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"kąpiel",null,{"v":225,"d":"liczba osób            225"},{"v":32,"d":"32 dm3/os d"},{"v":7.2,"d":"7.2 m3/d"},{"v":3,"d":"Nh=3.00"},{"v":1.8,"d":"Gsr=1.8 m3/h"},{"v":4,"d":"4.0 h"},{"v":5.4,"d":"Gmx=5.4 m3/h"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,150,null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":13.5,"d":"Vzs2.5= 13.5m3"},{"v":2000,"d":"2000dm3"},{"v":0.14814814814814814,"d":"fi=0.15"},{"v":0.5863978403990668,"d":"beta=0.59"},null,{"v":304.194,"d":"Qmx=304.2kW"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":20,"d":"dod%=20"},{"v":214.0544455948245,"d":"Qrd=214.1kW"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Rozbiory CW wg strażników"]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"Przeciętnie",null,"rano [w godz.   8:00 – 12:00]",{"v":70,"d":"70 os."}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"po południu           ",{"v":100,"d":"100 os."},"Mycie","Ładowanie"]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"wt  + śr + czw",null,"rano [w godz.   8:00 – 12:00]",{"v":70,"d":"70 os."},{"v":4,"d":"4 h"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"wiecz. [w godz.  15:00 – 19:00]",{"v":150,"d":"150 os."},{"v":4,"d":"4 h"},{"v":3,"d":"3 h"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"pon + pt",null,"rano [w godz.   8:00 – 12:00]","-"]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"wiecz. [w godz.  15:00 – 19:00]",{"v":100,"d":"100 os."}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":6},{"$error":"#NUM!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,"kąpiel",null,{"v":225,"d":"liczba osób            225"},{"v":45,"d":"45 dm3/os d"},{"v":10.125,"d":"10.1 m3/d"},{"v":3,"d":"Nh=3.00"},{"v":2.53125,"d":"Gsr=2.5 m3/h"},{"v":4,"d":"4 h"},{"v":7.59375,"d":"Gmx=7.6 m3/h"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},null,150,null,{"v":4,"d":"czas akumulacji            4.0"},{"v":30.375,"d":"Vzs2.5= 30.4m3"},{"v":2000,"d":"2000dm3"},{"v":0.06584362139917696,"d":"fi=0.07"},{"v":0.6622952508215144,"d":"beta=0.66"},null,{"v":427.77281250000004,"d":"Qmx=427.8kW"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":0,"d":"dod%=0"},{"v":283.3119021493122,"d":"Qrd=283.3kW"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"Obieg kotła CW",{"v":40,"d":"Dn40"},{"$error":"#REF!"},null,null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2012,null,"obliczenia","POZ",null,"NO-44","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",6,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":65,"d":"Dn65"},{"$error":"#VALUE!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":20,"d":"kvs=20.0"},"Dn50","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":12.5,"d":"kvs=12.5"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,402.5,null,"obieg CO Z1/1      / CW",{"v":50,"d":"Dn50"},{"$error":"#REF!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"obieg CO Z1/2 ",{"v":50,"d":"Dn50"},{"$error":"#REF!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"obieg CO Z2/1+Z2/2 ",{"v":65,"d":"Dn65"},{"$error":"#REF!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"obieg CO Z5",{"v":65,"d":"Dn65"},{"$error":"#REF!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",15,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,402.5,null,"obieg CW Z1/1      / cyrkulacja",{"v":40,"d":"Dn40"},{"$error":"#REF!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"obieg CW Z1/2      / cyrkulacja",{"v":40,"d":"Dn40"},{"$error":"#REF!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},{"$nulls":3},"obieg CW Z2/1+Z2/2       / cyrkulacja",{"v":50,"d":"Dn50"},{"$error":"#REF!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,"uzup 2012",null,"obieg CW Z5      / cyrkulacja",{"v":50,"d":"Dn50"},{"$error":"#REF!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,99,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn32",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":297,"d":"liczba osób            297"},{"v":65,"d":"65 dm3/os d"},{"v":19.305,"d":"19.3 m3/d"},{"v":2.323075575484444,"d":"Nh=2.32"},{"v":1.0725,"d":"Gsr=1.1 m3/h"},null,{"v":2.491498554707066,"d":"Gmx=2.5 m3/h"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,"82 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":6.228746386767665,"d":"Vzs2.5= 6.2m3"},{"v":720,"d":"720dm3"},{"v":0.11559308330959925,"d":"fi=0.12"},{"v":0.6679111642757559,"d":"beta=0.67"},null,{"v":140.35165025010394,"d":"Qmx=140.4kW"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"},null,2.7333333333333334,null,{"$error":"#REF!"},null,"jest V=2x500dm3",null,{"$error":"#REF!"},{"v":20,"d":"dod%=20"},{"v":112.49092095188473,"d":"Qrd=112.5kW"}]
["NO5",null,"mCW",2011,null,"obliczenia","POZ",null,"P002","OK",{"$error":"#N/A"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,30,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,{"v":3.64,"d":"3.6 os/m"},null,{"v":109.2,"d":"liczba osób            109"},{"v":65,"d":"65 dm3/os d"},{"v":7.098,"d":"7.1 m3/d"},{"v":2.9654430539109495,"d":"Nh=2.97"},{"v":0.3943333333333333,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.1693730442588843,"d":"Gmx=1.2 m3/h"},null,212.94]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.923432610647211,"d":"Vzs2.5= 2.9m3"},{"v":200,"d":"200dm3"},{"v":0.06841272799365898,"d":"fi=0.07"},{"v":0.6610348075753893,"d":"beta=0.66"},null,{"v":65.87338218986798,"d":"Qmx=65.9kW"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":50.07628829825238,"d":"Qrd=50.1kW"}]
["NO9",null,"mCW",2012,null,"obliczenia","POZ",null,"NO9-34","OK",{"$error":"#N/A"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,{"v":3.64,"d":"3.6 os/m"},null,{"v":182,"d":"liczba osób            182"},{"v":65,"d":"65 dm3/os d"},{"v":11.83,"d":"11.8 m3/d"},{"v":2.6179327956586604,"d":"Nh=2.62"},{"v":0.6572222222222223,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7205636095912198,"d":"Gmx=1.7 m3/h"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.301409023978049,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09299278393898708,"d":"fi=0.09"},{"v":0.6587172819263631,"d":"beta=0.66"},null,{"v":96.9231716029614,"d":"Qmx=96.9kW"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":15,"d":"dod%=15"},{"v":73.42171337708297,"d":"Qrd=73.4kW"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.1","OK",{"$error":"#N/A"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":25,"d":"Dn25"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,{"v":3.64,"d":"3.6 os/m"},null,{"v":182,"d":"liczba osób            182"},{"v":65,"d":"65 dm3/os d"},{"v":11.83,"d":"11.8 m3/d"},{"v":2.6179327956586604,"d":"Nh=2.62"},{"v":0.6572222222222223,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7205636095912198,"d":"Gmx=1.7 m3/h"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.301409023978049,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09299278393898708,"d":"fi=0.09"},{"v":0.6587172819263631,"d":"beta=0.66"},null,{"v":96.9231716029614,"d":"Qmx=96.9kW"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":15,"d":"dod%=15"},{"v":73.42171337708297,"d":"Qrd=73.4kW"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.4","OK",{"$error":"#N/A"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.5","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.5","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.5","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.5","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"}]
["Bole",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Bole 3.5","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$nulls":9},"OK",{"$error":"#N/A"},null,null,"Rozwiązanie alternatywne, tańsze ale z większym błędem pomiaru, wodomierz skrzydełkowy"]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":5,"d":"5.0 kPa"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":10,"d":"10.0 kPa"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,"zład",null,"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},null,5.6,null,"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1,"d":"wsp.b=1.0"},null,{"$error":"#REF!"}]
["Ko2012",null,"CO+CW",2012,null,"obliczenia","POZ",null,"Ko2012","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"v":6.16,"d":"6.2m3"},{"v":1.5,"d":"p1=1.5"},{"v":3.5,"d":"p2=3.5"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO","=",{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,{"v":3.4782608695652173,"d":"3.5 os/m"},null,{"v":156.52173913043478,"d":"liczba osób            157"},{"v":65,"d":"65 dm3/os d"},{"v":10.17391304347826,"d":"10.2 m3/d"},{"v":2.7160620920640444,"d":"Nh=2.72"},{"v":0.5652173913043478,"d":"Gsr=0.6 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.5351655302970684,"d":"Gmx=1.5 m3/h"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,"45 z 115",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.837913825742671,"d":"Vzs2.5= 3.8m3"},{"v":400,"d":"400dm3"},{"v":0.1042232885264422,"d":"fi=0.10"},{"v":0.6410082263919863,"d":"beta=0.64"},null,{"v":86.47928580059009,"d":"Qmx=86.5kW"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"},null,3.4782608695652173,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":63.74902365228423,"d":"Qrd=63.7kW"}]
["NO7",null,"mCW",2012,null,"obliczenia","POZ",null,"NO7-01","OK",{"$error":"#N/A"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,270.3,null,"różnica ","=",{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO","=",{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":25,"d":"Dn25"},{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,70,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,{"v":3.4782608695652173,"d":"3.5 os/m"},null,{"v":243.47826086956522,"d":"liczba osób            243"},{"v":65,"d":"65 dm3/os d"},{"v":15.82608695652174,"d":"15.8 m3/d"},{"v":2.438482402130238,"d":"Nh=2.44"},{"v":0.8792270531400966,"d":"Gsr=0.9 m3/h"},null,{"v":2.1439796965589535,"d":"Gmx=2.1 m3/h"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"70 z 115",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":5.359949241397384,"d":"Vzs2.5= 5.4m3"},{"v":400,"d":"400dm3"},{"v":0.07462757238643489,"d":"fi=0.07"},{"v":0.6916742787471237,"d":"beta=0.69"},null,{"v":120.77514070649156,"d":"Qmx=120.8kW"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,3.4782608695652173,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":10,"d":"dod%=10"},{"v":91.89076417261943,"d":"Qrd=91.9kW"}]
["NO7",null,"mCW","2012 anulowany",null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":16,"d":"kvs=16.0"},"Dn40","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.8,"d":"p1=1.8"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,70,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,{"v":3.4782608695652173,"d":"3.5 os/m"},null,{"v":243.47826086956522,"d":"liczba osób            243"},{"v":65,"d":"65 dm3/os d"},{"v":15.82608695652174,"d":"15.8 m3/d"},{"v":2.438482402130238,"d":"Nh=2.44"},{"v":0.8792270531400966,"d":"Gsr=0.9 m3/h"},{"v":18,"d":"18.0 h"},{"v":2.1439796965589535,"d":"Gmx=2.1 m3/h"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":5.359949241397384,"d":"Vzs2.5= 5.4m3"},{"v":500,"d":"500dm3"},{"v":0.0932844654830436,"d":"fi=0.09"},{"v":0.6739852425676229,"d":"beta=0.67"},null,{"v":120.77514070649156,"d":"Qmx=120.8kW"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"},null,3.4782608695652173,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":89.54072875572385,"d":"Qrd=89.5kW"}]
["NO7",null,"CO+CW",2012,null,"obliczenia","POZ",null,"NO7-02","OK",{"$error":"#N/A"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,{"v":3.64,"d":"3.6 os/m"},null,{"v":182,"d":"liczba osób            182"},{"v":65,"d":"65 dm3/os d"},{"v":11.83,"d":"11.8 m3/d"},{"v":2.6179327956586604,"d":"Nh=2.62"},{"v":0.6572222222222223,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7205636095912198,"d":"Gmx=1.7 m3/h"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.301409023978049,"d":"Vzs2.5= 4.3m3"},{"v":300,"d":"300dm3"},{"v":0.0697445879542403,"d":"fi=0.07"},{"v":0.6824006442331016,"d":"beta=0.68"},null,{"v":96.9231716029614,"d":"Qmx=96.9kW"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":76.06149995442277,"d":"Qrd=76.1kW"}]
["NO3",null,"KG+GAZ",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},{"$nulls":3},"Obieg kotła CW",{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"}]
["NO3",null,"KG+GAZ",2013,null,"obliczenia","POZ",null,"No-0082 ","KG",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",6,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[{"$nulls":8},"No-0082 ",null,{"$error":"#N/A"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,{"v":3.64,"d":"3.6 os/m"},null,{"v":140,"d":"liczba osób            140"},{"v":65,"d":"65 dm3/os d"},{"v":9.1,"d":"9.1 m3/d"},{"v":2.7910053671725255,"d":"Nh=2.79"},{"v":0.5055555555555555,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.4110082689594434,"d":"Gmx=1.4 m3/h"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.527520672398609,"d":"Vzs2.5= 3.5m3"},{"v":400,"d":"400dm3"},{"v":0.11339409096304798,"d":"fi=0.11"},{"v":0.6276221658619892,"d":"beta=0.63"},null,{"v":79.48523136441648,"d":"Qmx=79.5kW"}]
["NO10",null,"mCW",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":57.369697022422834,"d":"Qrd=57.4kW"}]
["NO3",null,"KG+GAZ",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},{"$nulls":3},"Obieg kotła CW",{"v":32,"d":"Dn32"},{"$error":"#REF!"},null,null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO3",null,"KG+GAZ",2013,null,"obliczenia","POZ",null,"NO-0083","KG",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",6,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,"-"]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":4,"d":"4.0 kPa"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO10",null,"CO","2012 wykonane",null,"obliczenia","POZ",null,"No-0084","OK",{"$error":"#N/A"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":125,"d":"Dn125"},{"$error":"#VALUE!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":65,"d":"kvs=65.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},"lato",{"v":1,"d":"1 szt"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":125,"d":"Dn125"},{"$error":"#VALUE!"},null,{"v":150,"d":"Dn150"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":25,"d":"kvs=25.0"},"Dn50","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},{"v":5,"d":"5 szt"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",11,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":80,"d":"Dn80"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"   z.reg CO ",{"v":25,"d":"kvs=25.0"},"Dn50","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},{"v":1,"d":"1 szt"},"NG18/"]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":65,"d":"Dn65"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"   z.reg CO",{"v":25,"d":"kvs=25.0"},"Dn50","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},{"v":1,"d":"1 szt"},"NG18/"]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":100,"d":"Dn100"},{"$error":"#VALUE!"},null,{"v":100,"d":"Dn100"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"v":80,"d":"Dn80"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"}]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},"   z.reg CO",{"v":25,"d":"kvs=25.0"},"Dn50","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},{"v":2,"d":"2 szt"},"NG18/"]
["NO10",null,"CO+CW+CT",2012,null,"obliczenia","POZ",null,"eXo0015","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"v":100,"d":"Dn100"},{"$error":"#REF!"}]
[{"$nulls":10},{"$error":"#N/A"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},null,"115 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-04","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},null,"123 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-05","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},null,"130 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-06","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0114","Wym",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2012-12-04"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-07","Wym",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},null,2.488888888888889,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"NO7-08","Wym",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m60","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,109,null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},null,1.8166666666666667,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":69.5096238954669,"d":"Qrd=69.5kW"},null,null,"2012-02-01"]
["mCW-13+14","m60",null,2013,null,"obliczenia","POZ",null,"NO7-09","Wym",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,30,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":90,"d":"liczba osób            90"},{"v":65,"d":"65 dm3/os d"},{"v":5.85,"d":"5.9 m3/d"},{"v":3.108713792604074,"d":"Nh=3.11"},{"v":0.32499999999999996,"d":"Gsr=0.3 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.010331982596324,"d":"Gmx=1.0 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,"82 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.52582995649081,"d":"Vzs2.5= 2.5m3"},{"v":250,"d":"250dm3"},{"v":0.09897736756093051,"d":"fi=0.10"},{"v":0.6195296014329351,"d":"beta=0.62"},null,{"v":56.91424576183448,"d":"Qmx=56.9kW"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},null,2.7333333333333334,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":38.786065991953976,"d":"Qrd=38.8kW"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-10","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,30,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":90,"d":"liczba osób            90"},{"v":65,"d":"65 dm3/os d"},{"v":5.85,"d":"5.9 m3/d"},{"v":3.108713792604074,"d":"Nh=3.11"},{"v":0.32499999999999996,"d":"Gsr=0.3 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.010331982596324,"d":"Gmx=1.0 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.52582995649081,"d":"Vzs2.5= 2.5m3"},{"v":250,"d":"250dm3"},{"v":0.09897736756093051,"d":"fi=0.10"},{"v":0.6195296014329351,"d":"beta=0.62"},null,{"v":56.91424576183448,"d":"Qmx=56.9kW"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":38.786065991953976,"d":"Qrd=38.8kW"},null,null,"2012-02-01"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"NO7-11","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":150,"d":"liczba osób            150"},{"v":65,"d":"65 dm3/os d"},{"v":9.75,"d":"9.8 m3/d"},{"v":2.7444141202581362,"d":"Nh=2.74"},{"v":0.5416666666666666,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.486557648473157,"d":"Gmx=1.5 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.716394121182893,"d":"Vzs2.5= 3.7m3"},{"v":400,"d":"400dm3"},{"v":0.10763121104945776,"d":"fi=0.11"},{"v":0.6359303259046551,"d":"beta=0.64"},null,{"v":83.741095799934,"d":"Qmx=83.7kW"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":58.57885257803148,"d":"Qrd=58.6kW"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"NO7-12","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},null,"115 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0111","OK",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},null,"115 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0112","OK",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},null,"115 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0113","OK",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m30","CO+CW",2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,30,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":90,"d":"liczba osób            90"},{"v":65,"d":"65 dm3/os d"},{"v":5.85,"d":"5.9 m3/d"},{"v":3.108713792604074,"d":"Nh=3.11"},{"v":0.32499999999999996,"d":"Gsr=0.3 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.010331982596324,"d":"Gmx=1.0 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.52582995649081,"d":"Vzs2.5= 2.5m3"},{"v":250,"d":"250dm3"},{"v":0.09897736756093051,"d":"fi=0.10"},{"v":0.6195296014329351,"d":"beta=0.62"},null,{"v":56.91424576183448,"d":"Qmx=56.9kW"},null,null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":38.786065991953976,"d":"Qrd=38.8kW"},null,null,"2012-12-04"]
["mCW-13+14","m30",null,2013,null,"obliczenia","POZ",null,"No-0115","OK",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["NO2",null,"CO [bez cw]","2012 wykonane",null,"obliczenia","POZ",null,"NO_04","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO [bez cw]","2012 wykonane",null,"obliczenia","POZ",null,"NO_04","OK",{"$error":"#N/A"},{"$nulls":3},"różnica ",{"v":6.3,"d":"kvs=6.3"},"zima",{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["NO2",null,"CO [bez cw]","2012 wykonane",null,"obliczenia","POZ",null,"NO_04","OK",{"$error":"#N/A"},{"$nulls":3},"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"}]
["NO2",null,"CO [bez cw]","2012 wykonane",null,"obliczenia","POZ",null,"NO_04","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"zima",{"$error":"#VALUE!"},null,{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"}]
["NO2",null,"CO [bez cw]","2012 wykonane",null,"obliczenia","POZ",null,"NO_04","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},null,"115 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-12-04"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0116","OK",{"$error":"#N/A"},{"$nulls":12},"2012-12-04"]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m45","CO+CW",2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,45,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":135,"d":"liczba osób            135"},{"v":65,"d":"65 dm3/os d"},{"v":8.775,"d":"8.8 m3/d"},{"v":2.81588213727366,"d":"Nh=2.82"},{"v":0.48750000000000004,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.3727425419209094,"d":"Gmx=1.4 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.4318563548022736,"d":"Vzs2.5= 3.4m3"},{"v":300,"d":"300dm3"},{"v":0.0874162461899675,"d":"fi=0.09"},{"v":0.6493521164021383,"d":"beta=0.65"},null,{"v":77.32963792538688,"d":"Qmx=77.3kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":55.23558045220714,"d":"Qrd=55.2kW"},null,null,"2012-02-01"]
["mCW-13+14","m45",null,2013,null,"obliczenia","POZ",null,"No-0118","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m50","CO+CW",2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":1000,"d":"kvs=1000.0"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":150,"d":"liczba osób            150"},{"v":65,"d":"65 dm3/os d"},{"v":9.75,"d":"9.8 m3/d"},{"v":2.7444141202581362,"d":"Nh=2.74"},{"v":0.5416666666666666,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.486557648473157,"d":"Gmx=1.5 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.716394121182893,"d":"Vzs2.5= 3.7m3"},{"v":400,"d":"400dm3"},{"v":0.10763121104945776,"d":"fi=0.11"},{"v":0.6359303259046551,"d":"beta=0.64"},null,{"v":83.741095799934,"d":"Qmx=83.7kW"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":58.57885257803148,"d":"Qrd=58.6kW"},null,null,"2012-02-01"]
["mCW-13+14","m50",null,2013,null,"obliczenia","POZ",null,"No-0119","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["mCW-13+14","m40","CO+CW",2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["mCW-13+14","m40","CO+CW",2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["mCW-13+14","m40","CO+CW",2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m40","CO+CW",2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["mCW-13+14","m40","CO+CW",2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["mCW-13+14","m40","CO+CW",2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,40,null,"z.reg CW",{"v":6.3,"d":"kvs=6.3"},"Dn20",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":120,"d":"liczba osób            120"},{"v":65,"d":"65 dm3/os d"},{"v":7.8,"d":"7.8 m3/d"},{"v":2.897982031181138,"d":"Nh=2.90"},{"v":0.43333333333333335,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.2557922135118265,"d":"Gmx=1.3 m3/h"},null,null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.139480533779566,"d":"Vzs2.5= 3.1m3"},{"v":300,"d":"300dm3"},{"v":0.09555720979063857,"d":"fi=0.10"},{"v":0.6358651268776184,"d":"beta=0.64"},null,{"v":70.74156603648454,"d":"Qmx=70.7kW"},null,null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":10,"d":"dod%=10"},{"v":49.480304349641735,"d":"Qrd=49.5kW"},null,null,"2012-02-01"]
["mCW-13+14","m40",null,2013,null,"obliczenia","POZ",null,"No-0120","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#VALUE!"},{"$nulls":3},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#VALUE!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#VALUE!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,50,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn32",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,{"v":2.5,"d":"2.5 os/m"},null,{"v":125,"d":"liczba osób            125"},{"v":65,"d":"65 dm3/os d"},{"v":8.125,"d":"8.1 m3/d"},{"v":2.869259770435793,"d":"Nh=2.87"},{"v":0.4513888888888889,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.295151979710601,"d":"Gmx=1.3 m3/h"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.2378799492765027,"d":"Vzs2.5= 3.2m3"},{"v":300,"d":"300dm3"},{"v":0.09265321898887398,"d":"fi=0.09"},{"v":0.6405695072749826,"d":"beta=0.64"},null,{"v":72.95878913260864,"d":"Qmx=73.0kW"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":53.745451946962646,"d":"Qrd=53.7kW"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0122","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,40,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":120,"d":"liczba osób            120"},{"v":65,"d":"65 dm3/os d"},{"v":7.8,"d":"7.8 m3/d"},{"v":2.897982031181138,"d":"Nh=2.90"},{"v":0.43333333333333335,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.2557922135118265,"d":"Gmx=1.3 m3/h"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.139480533779566,"d":"Vzs2.5= 3.1m3"},{"v":300,"d":"300dm3"},{"v":0.09555720979063857,"d":"fi=0.10"},{"v":0.6358651268776184,"d":"beta=0.64"},null,{"v":70.74156603648454,"d":"Qmx=70.7kW"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":51.72940909280726,"d":"Qrd=51.7kW"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0123","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"Zawór reg CO/CT MAX",null,null,{"$error":"#VALUE!"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"Licznik ciepła",null,null,{"v":0,"d":"0.0 kPa"}]
["NO10",null,"CO+CW",2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"Przewody",null,null,{"v":7,"d":"7.0 kPa"}]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},{"$nulls":3},"Przyłącze","=",{"$error":"#VALUE!"},{"$nulls":6},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,0.85,null,"sieć  CO/     inst CO","=",{"$error":"#VALUE!"},null,"=",{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#REF!"},null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,40,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,{"v":3,"d":"3.0 os/m"},null,{"v":120,"d":"liczba osób            120"},{"v":65,"d":"65 dm3/os d"},{"v":7.8,"d":"7.8 m3/d"},{"v":2.897982031181138,"d":"Nh=2.90"},{"v":0.43333333333333335,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.2557922135118265,"d":"Gmx=1.3 m3/h"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,"182 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.139480533779566,"d":"Vzs2.5= 3.1m3"},{"v":300,"d":"300dm3"},{"v":0.09555720979063857,"d":"fi=0.10"},{"v":0.6358651268776184,"d":"beta=0.64"},null,{"v":70.74156603648454,"d":"Qmx=70.7kW"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},null,3.64,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":51.72940909280726,"d":"Qrd=51.7kW"},null,null,"2012-02-01"]
[{"$nulls":3},2013,null,"obliczenia","POZ",null,"No-0124","OK",{"$error":"#N/A"},{"$nulls":12},"2012-02-01"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0131","OK","Wita Stwosza 1 ",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0131",null,"Wita Stwosza 1 ",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0132","OK","Wita Stwosza 2",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,0.85,null,"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0132",null,"Wita Stwosza 2",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0133","OK","Wita Stwosza 4 ",{"$nulls":4},4,{"$nulls":7},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0133",null,"Wita Stwosza 4 ",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134","OK","Wita Stwosza 10",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,49,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,{"v":3,"d":"3.0 os/m"},null,{"v":147,"d":"liczba osób            147"},{"v":65,"d":"65 dm3/os d"},{"v":9.555,"d":"9.6 m3/d"},{"v":2.7579760004086795,"d":"Nh=2.76"},{"v":0.5308333333333333,"d":"Gsr=0.5 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.464025593550274,"d":"Gmx=1.5 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":3.660063983875685,"d":"Vzs2.5= 3.7m3"},{"v":500,"d":"500dm3"},{"v":0.13660963365742695,"d":"fi=0.14"},{"v":0.6124811872894587,"d":"beta=0.61"},null,{"v":82.47181507489483,"d":"Qmx=82.5kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":5,"d":"dod%=5"},{"v":53.03805697573768,"d":"Qrd=53.0kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0134",null,"Wita Stwosza 10",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0135","OK","Drużbackiej 1-3",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0135",null,"Drużbackiej 1-3",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136","OK","Narutowicza 7",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":15,"d":"Dn15"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,15,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,{"v":3,"d":"3.0 os/m"},null,{"v":45,"d":"liczba osób            45"},{"v":65,"d":"65 dm3/os d"},{"v":2.925,"d":"2.9 m3/d"},{"v":3.681561493958846,"d":"Nh=3.68"},{"v":0.16249999999999998,"d":"Gsr=0.2 m3/h"},{"v":18,"d":"18.0 h"},{"v":0.5982537427683124,"d":"Gmx=0.6 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":1.495634356920781,"d":"Vzs2.5= 1.5m3"},{"v":250,"d":"250dm3"},{"v":0.16715315400663913,"d":"fi=0.17"},{"v":0.5342698587315924,"d":"beta=0.53"},null,{"v":33.70096278290076,"d":"Qmx=33.7kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":15,"d":"dod%=15"},{"v":20.706219918909895,"d":"Qrd=20.7kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0136",null,"Narutowicza 7",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0137","OK","Narutowicza 15",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,0.85,null,"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0137",null,"Narutowicza 15",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0138","OK","Narutowicza 20",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0138",null,"Narutowicza 20",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0139","OK","Wita Stwosza 6",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",{"$nulls":3},"Przyłącze",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,270.3,null,"różnica ",{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,0.85,null,"sieć  CO/     inst CO",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",{"$nulls":3},"z.reg CO",{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0139",null,"Wita Stwosza 6",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0140","OK","Narutowicza 6 nowy",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,0.85,null,"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",{"$nulls":3},"z.reg CO",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0140",null,"Narutowicza 6 nowy",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0141","OK","Narutowicza 6 stary",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",{"$nulls":3},"z.reg CO",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0141",null,"Narutowicza 6 stary",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0142","OK","Narutowicza 6 b-m",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",{"$nulls":3},"Przyłącze",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",{"$nulls":3},"z.reg CO",{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0142",null,"Narutowicza 6 b-m",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0144","OK","Krakowska 40",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",{"$nulls":3},"Przyłącze",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,0.85,null,"sieć  CO/     inst CO",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",{"$nulls":3},"z.reg CO",{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",10,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0144",null,"Krakowska 40",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0145","OK","Krakowska 42",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,0.85,null,"sieć  CO/     inst CO",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},null,{"v":65,"d":"Dn65"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",{"$nulls":3},"z.reg CO",{"v":10,"d":"kvs=10.0"},"Dn32","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0145",null,"Krakowska 42",{"$nulls":12},"2013-05-15"]
[]
[]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147","OK","Krakowska 32",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":15,"d":"Dn15"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":200,"d":"200dm3"},{"v":0.046886434647365055,"d":"fi=0.05"},{"v":0.7119380278586542,"d":"beta=0.71"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":5,"d":"dod%=5"},{"v":71.85072453503794,"d":"Qrd=71.9kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0147",null,"Krakowska 32",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0148","OK","Bandrowskiego 4",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",{"$nulls":3},"Przyłącze",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,270.3,null,"różnica ",{"v":12.5,"d":"kvs=12.5"},"Dn32","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,0.85,null,"sieć  CO/     inst CO",{"v":50,"d":"Dn50"},{"$error":"#VALUE!"},null,{"v":80,"d":"Dn80"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",{"$nulls":3},"z.reg CO",{"v":12.5,"d":"kvs=12.5"},{"$error":"#N/A"},"zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":400,"d":"400dm3"},{"v":0.09377286929473011,"d":"fi=0.09"},{"v":0.6574346531677959,"d":"beta=0.66"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"v":66.35009553658203,"d":"Qrd=66.4kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0148",null,"Bandrowskiego 4",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Zawór różnicy ciśnień",null,null,{"v":4,"d":"4.0 kPa"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Opory wymiennika CO",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Zawór regulacyjny CO",null,null,{"$error":"#REF!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Opory wymiennika CW",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Zawór regulacyjny CW",null,null,{"v":15,"d":"15.0 kPa"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"Przyłącze",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",{"$nulls":3},"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0149","OK","Klikowska 31 Pyrek",{"$nulls":3},"sieć  CO/     inst CO",{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"}]
["No2013","m61","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"z.reg CO",{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1,"d":"wsp.b=1.0"},null,{"$error":"#REF!"}]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"Podmieszanie CO niski parametr",{"$nulls":3},{"v":20,"d":"Dn20"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":4},{"v":2.5,"d":"kvs=2.5"},"Dn15","zima",{"$error":"#REF!"},{"$nulls":4},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},{"$error":"#REF!"},{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"v":15,"d":"Dn15"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},"z.reg CW",{"v":4,"d":"kvs=4.0"},{"$nulls":3},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",null,"302 aaa",null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},{"v":100,"d":"100dm3"},{"v":0.023443217323682528,"d":"fi=0.02"},{"v":0.757769720255427,"d":"beta=0.76"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0149",null,"Klikowska 31 Pyrek",{"$nulls":3},{"v":0,"d":"Pojemność cieplna  0"},{"$nulls":3},{"v":0,"d":"czas ład= 0min"},{"v":50,"d":"dod%=50"},{"v":109.25169105925733,"d":"Qrd=109.3kW"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154","OK","Zielone 29 wz_1",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":15,"d":"Dn15"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,28,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,{"v":3,"d":"3.0 os/m"},null,{"v":84,"d":"liczba osób            84"},{"v":65,"d":"65 dm3/os d"},{"v":5.46,"d":"5.5 m3/d"},{"v":3.1614896659054983,"d":"Nh=3.16"},{"v":0.30333333333333334,"d":"Gsr=0.3 m3/h"},{"v":18,"d":"18.0 h"},{"v":0.9589851986580011,"d":"Gmx=1.0 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.397462996645003,"d":"Vzs2.5= 2.4m3"},{"v":300,"d":"300dm3"},{"v":0.1251322754177305,"d":"fi=0.13"},{"v":0.5933659589667069,"d":"beta=0.59"},null,{"v":54.021767318624455,"d":"Qmx=54.0kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":5,"d":"dod%=5"},{"v":33.6574116585965,"d":"Qrd=33.7kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0154",null,"Zielone 29 wz_1",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155","OK","Zielone 29 wz_2",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",{"$nulls":3},"Przyłącze",{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,270.3,null,"różnica ",{"v":8,"d":"kvs=8.0"},"Dn25","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,0.85,null,"sieć  CO/     inst CO",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":20,"d":"Dn20"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,36,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,{"v":3,"d":"3.0 os/m"},null,{"v":108,"d":"liczba osób            108"},{"v":65,"d":"65 dm3/os d"},{"v":7.02,"d":"7.0 m3/d"},{"v":2.973449150952281,"d":"Nh=2.97"},{"v":0.38999999999999996,"d":"Gsr=0.4 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.1596451688713894,"d":"Gmx=1.2 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.8991129221784733,"d":"Vzs2.5= 2.9m3"},{"v":300,"d":"300dm3"},{"v":0.10347992922420274,"d":"fi=0.10"},{"v":0.6235741364969543,"d":"beta=0.62"},null,{"v":65.32538935178952,"d":"Qmx=65.3kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":5,"d":"dod%=5"},{"v":42.77198441918796,"d":"Qrd=42.8kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0155",null,"Zielone 29 wz_2",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0157","OK","Sanguszków 20A",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",{"$nulls":3},"Przyłącze",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},"=",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0157",null,"Sanguszków 20A",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160","OK","Skargi 37",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":32,"d":"Dn32"},{"$error":"#REF!"},{"v":15,"d":"Dn15"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,28,null,"z.reg CW",{"v":4,"d":"kvs=4.0"},"Dn15",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,{"v":3,"d":"3.0 os/m"},null,{"v":84,"d":"liczba osób            84"},{"v":65,"d":"65 dm3/os d"},{"v":5.46,"d":"5.5 m3/d"},{"v":3.1614896659054983,"d":"Nh=3.16"},{"v":0.30333333333333334,"d":"Gsr=0.3 m3/h"},{"v":18,"d":"18.0 h"},{"v":0.9589851986580011,"d":"Gmx=1.0 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":2.397462996645003,"d":"Vzs2.5= 2.4m3"},{"v":300,"d":"300dm3"},{"v":0.1251322754177305,"d":"fi=0.13"},{"v":0.5933659589667069,"d":"beta=0.59"},null,{"v":54.021767318624455,"d":"Qmx=54.0kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",null,3.1,null,{"$error":"#REF!"},{"$nulls":3},{"$error":"#REF!"},{"v":5,"d":"dod%=5"},{"v":33.6574116585965,"d":"Qrd=33.7kW"},null,null,"2013-05-15"]
["No2013","m60","CO+CW",2013,null,"obliczenia","POZ",null,"No-0160",null,"Skargi 37",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0162","OK","Węzeł wiszący CO wersja A i B",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",{"$nulls":3},"Przyłącze",{"v":15,"d":"Dn15"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,270.3,null,"różnica ",{"v":1.6,"d":"kvs=1.6"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,0.85,null,"sieć  CO/     inst CO",{"v":15,"d":"Dn15"},{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",{"$nulls":3},"z.reg CO",{"v":1.6,"d":"kvs=1.6"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":1.5,"d":"p1=1.5"},{"v":3,"d":"p2=3.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},"=",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0162",null,"Węzeł wiszący CO wersja A i B",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0163","OK","Tarnovia węzeł + przepompownia",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",{"$nulls":3},"Przyłącze",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,270.3,null,"różnica ",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},"=",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0163",null,"Tarnovia węzeł + przepompownia",{"$nulls":12},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Zawór różnicy ciśnień",null,null,{"$error":"#VALUE!"},{"$nulls":4},"pompa c.o.",{"$error":"#REF!"},null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",{"$nulls":7},"maksymalny opór zaworu",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Opory wymiennika CO",null,null,{"v":15,"d":"15.0 kPa"},null,{"v":10,"d":"10.0 kPa"},"V max sieć",null,{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Zawór regulacyjny CO",null,null,{"$error":"#VALUE!"},null,null,"V max instal CO/ CW",null,{"$error":"#REF!"},null,null,"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Opory wymiennika CW",null,null,{"v":20,"d":"20.0 kPa"},null,{"v":20,"d":"20.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Zawór regulacyjny CW",null,null,{"$error":"#VALUE!"},{"$nulls":7},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Licznik ciepła CW/CO",null,null,{"v":7,"d":"7.0 kPa"},null,{"v":5,"d":"5.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",null,"Przewody",null,null,{"v":10,"d":"10.0 kPa"},null,{"v":15,"d":"15.0 kPa"},{"$nulls":5},"2013-05-15"]
["No2013","typ A","CO",2013,null,"obliczenia","POZ",null,"No-0166","OK","Kochanowskiego 30 Intech",{"$nulls":12},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":3},"Przyłącze",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":6},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,270.3,null,"różnica ",{"v":6.3,"d":"kvs=6.3"},"Dn20","zima",{"$error":"#VALUE!"},"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,{"$error":"#REF!"},"-",{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,{"$error":"#REF!"},"-",{"$error":"#VALUE!"},null,{"v":25,"d":"Dn25"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":50,"d":"Dn50"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,{"$error":"#REF!"},{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":3},"z.reg CO",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":3},"z.reg CT",{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,null,{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":4},{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,"NG18/",null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,null,{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":4},{"v":4,"d":"kvs=4.0"},"Dn15","zima",{"$error":"#VALUE!"},{"v":1.1,"d":"wsp.b=1.1"},null,{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,0.85,null,"sieć  CO/     inst CO",{"v":25,"d":"Dn25"},{"$error":"#VALUE!"},null,{"v":40,"d":"Dn40"},{"$error":"#REF!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":3},"przeponowe naczynie wzbiorcze CO",13.5,{"$error":"#REF!"},{"v":2,"d":"p1=2.0"},{"v":4,"d":"p2=4.0"},{"$error":"#REF!"},{"$error":"#REF!"},{"$error":"#REF!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":3},"sieć CW/   ładowanie CW",{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},null,{"v":32,"d":"Dn32"},{"$error":"#VALUE!"},{"$nulls":3},"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,"uzup 2012",null,"rozładowanie CW/   cyrkulacja CW",{"$nulls":3},{"v":40,"d":"Dn40"},{"$error":"#VALUE!"},{"v":20,"d":"Dn20"},{"$error":"#VALUE!"},null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,60,null,"z.reg CW",{"v":10,"d":"kvs=10.0"},"Dn25",{"$error":"#VALUE!"},null,"lato",{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,{"v":3,"d":"3.0 os/m"},null,{"v":180,"d":"liczba osób            180"},{"v":65,"d":"65 dm3/os d"},{"v":11.7,"d":"11.7 m3/d"},{"v":2.6250006852214307,"d":"Nh=2.63"},{"v":0.6499999999999999,"d":"Gsr=0.7 m3/h"},{"v":18,"d":"18.0 h"},{"v":1.7062504453939298,"d":"Gmx=1.7 m3/h"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,"93 os wg KW",null,{"v":2.5,"d":"czas akumulacji            2.5"},{"v":4.265626113484824,"d":"Vzs2.5= 4.3m3"},"=",{"$error":"#VALUE!"},{"$error":"#VALUE!"},null,{"v":96.11687925669649,"d":"Qmx=96.1kW"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",null,3.1,null,{"$error":"#VALUE!"},{"$nulls":3},{"$error":"#VALUE!"},{"v":5,"d":"dod%=5"},{"$error":"#VALUE!"},null,null,"2013-05-15"]
["No2013","m60","CO",2013,null,"obliczenia","POZ",null,"No-0166",null,"Kochanowskiego 30 Intech",{"$nulls":12},"2013-05-15"]
["End","End","End","End","End","End","End","End","End","End",null,"End","End","End","End","End","End","End","End","End","End","End","End"]
[{"$nulls":23},"End"]

{"sheet":"Katalog","index":1,"n_rows":134,"n_cols":31,"rows_kept":134,"flags":["formulas_cached_only"]}
[]
[null,"MENU  Dane/ Definiuj zakres"]
[{"$nulls":23},"SIEĆ ZEWNĘTRZNA K.MIARKI",null,null,"średnica ","Moc","Dp / metr","długość","spadek Pa"]
[{"$nulls":24},"Temp 90/70",null,"125x11,4",300,17,60,1020]
["46-7","46-6",{"$nulls":3},3226,{"$nulls":5},3222,{"$nulls":3},512,{"$nulls":10},"110x10",100,5,132,660]
[1.6,1.6,"Dn15",null,null,1.6,"Dn15",{"$nulls":4},1.6,"Dn15",null,null,4.1,"Dn15/20",{"$nulls":3},"Dobory"]
[2.5,2.5,"Dn15",null,null,2.5,"Dn15",{"$nulls":4},2.5,"Dn15",null,null,16,"Dn25/32",{"$nulls":3},"Pompa",{"$nulls":5},"63x5,8",160,150,10,1500]
[4,4,"Dn15",null,null,4,"Dn15",{"$nulls":4},4,"Dn15",null,null,35,"Dn40/50",{"$nulls":9},"40x3,7",72,320,32,10240]
[6.3,6.3,"Dn20",null,null,6.3,"Dn20",{"$nulls":4},6.3,"Dn20",null,null,70,"Dn65",{"$nulls":3},"Karola Miarki",{"$nulls":8},"suma",13.42]
[8,8,"Dn25",null,null,10,"Dn25",{"$nulls":4},8,"Dn25",{"$nulls":6},"spadek licznik",10]
[12.5,12.5,"Dn32",null,null,16,"Dn32",{"$nulls":4},10,"Dn32",{"$nulls":6},"spadek wymiennik",10]
[16,16,"Dn40",null,null,25,"Dn40",{"$nulls":4},16,"Dn40",{"$nulls":6},"spadek węzeł",10]
[20,20,"Dn50",null,null,40,"Dn50",{"$nulls":4},25,"Dn50",{"$nulls":6},"spadek sieć zewnętrzna",20]
[{"$nulls":12},"Dn40",{"$nulls":6},"Spadek instalacja wewnętrzna",30]
[{"$nulls":12},"Dn50",{"$nulls":6},"zapas",20]
[]
[null,"46-6",8,"Dn25",null,3226,40,null,"Dn50",null,null,3222,6.3,null,"Dn20",{"$nulls":4},"Sumaryczny spadek"]
[{"$nulls":19},"SPADEK",100,"kPa"]
[{"$nulls":19},"PRZEPŁYW",13.3,"m3/h"]
[null,"f[x] wyszukaj.pionowo"]
[null,"wartość pierwsza kolumna"]
[null,"nr kolumny z której czyta"]
[null,"sortowanie tak/nie jezli nie to jeśli nie znajdzie znajduje bład"]
[{"$nulls":10},"naczNWCW"]
[null,"Ws","wodomierz wielostrumieniowy =zmiana na JS",{"$nulls":7},"NWCW","naczynie wzbiorcze CW wg zasobnika"]
[null,"Qn=1,5",null,"Dn15","Ws130-1,5","Ws-1,5",{"$nulls":4},100,null,"V=12 dm3",null,"typ DD12/4",1]
[null,"Qn=2,5",null,"Dn20","Ws120-2,5","Ws-2,5",{"$nulls":4},150,null,"V=18 dm3",null,"typ DD18/4",1]
[null,"Qn=3,5",null,"Dn25","Ws120-3,5","Ws-3,5",{"$nulls":4},200,null,"V=18 dm3",null,"typ DD18/4",1]
[null,"Qn=6",null,"Dn32","Ws120-6","Ws-6",{"$nulls":4},250,null,"V=25 dm3",null,"typ DD25/4",1]
[null,"Qn=10",null,"Dn40","Ws120-10","Ws-10",{"$nulls":4},300,null,"V=25 dm3",null,"typ DD25/4",1]
[{"$nulls":10},400,null,"V=33 dm3",null,"typ DD33/4",1]
[null,"Ws","Qn=2,5","Ws120-2,5",{"$nulls":6},500,null,"V=45 dm3",null,"typ DD25/4",2]
[{"$nulls":10},720,null,"V=60 dm3",null,"typ DD33/4",2]
[null,"Js","wodomierz jednostrumieniowy ",{"$nulls":7},1000,null,"V=100 dm3",null,"typ DT5 100/4 KSB",1]
[null,"Q3= 1,6 m3/h",null,"Dn15","Js90-1,5","Js-1,5",{"$nulls":4},1500,null,"V=200 dm3",null,"typ DT5 200/4 KSB",1]
[null,"Q3= 2,5 m3/h",null,"Dn15","Js90-1,5","Js-1,5",{"$nulls":4},2000,null,"V=200 dm3",null,"typ DT5 200/4 KSB",1]
[null,"Q3= 4 m3/h",null,"Dn20","Js90-2,5","Js-2,5",{"$nulls":4},3000,null,"V=300 dm3",null,"typ DT5 300/4 KSB",1]
[null,"Q3= 6.3 m3/h",null,"Dn25","Js90-3,5","Js-3,5"]
[null,"Q3= 10 m3/h",null,"Dn32","Js90-6","Js-6",{"$nulls":4},"DD/ DT5",720,0,null,"typ DD33/4"]
[null,"Q3= 16 m3/h",null,"Dn40","Js90-10","Js-10"]
[null,"Q3= 25 m3/h",null,"Dn50","Js90-15","Js-15"]
[]
[null,"Js","Q3= 1,6 m3/h",{"$error":"#N/A"},{"$error":"#N/A"},{"$nulls":7},"Termometr bimetaliczny mocowany w osłonie"]
[{"$nulls":11},"Term_bim","Termometr bimetaliczny mocowany bezpośrednio"]
[null,"Kamstrup","licznik ciepła",{"$nulls":5},"Wymiary WIKA katalog",{"$nulls":3},"gwint WP",null,"osłona NP"]
[null,0,1.5,"xx",{"$nulls":4},"czujnik",null,"osłona",{"v":15,"d":"Dn15"},"czujnik L=45mm",null,"osłona L=40mm",{"v":32.5,"d":"33"}]
[null,1.5,2.5,"Dn20",{"$nulls":4},45,null,40,{"v":20,"d":"Dn20"},"czujnik L=45mm",null,"osłona L=40mm",35]
[null,2.5,3.5,"Dn20",{"$nulls":4},63,null,60,{"v":25,"d":"Dn25"},"czujnik L=45mm",null,"osłona L=40mm",{"v":37.5,"d":"38"}]
[null,3.5,6,"Dn25",{"$nulls":4},100,null,100,{"v":32,"d":"Dn32"},"czujnik L=45mm",null,"osłona L=40mm",41]
[null,6,10,"Dn25",{"$nulls":4},140,null,160,{"v":40,"d":"Dn40"},"czujnik L=45mm",null,"osłona L=60mm",45]
[null,10,15,"Dn40",{"$nulls":4},160,null,200,{"v":50,"d":"Dn50"},"czujnik L=63mm",null,"osłona L=60mm",50]
[null,15,25,"Dn50",{"$nulls":4},200,null,250,{"v":65,"d":"Dn65"},"czujnik L=63mm",null,"osłona L=60mm",{"v":57.5,"d":"58"}]
[null,25,40,"Dn65",{"$nulls":4},240,null,300,{"v":80,"d":"Dn80"},"czujnik L=63mm",null,"osłona L=60mm",65]
[null,40,60,"Dn80",{"$nulls":4},290,null,null,{"v":100,"d":"Dn100"},"czujnik L=100mm",null,"osłona L=100mm",75]
[null,60,100,"Dn100",{"$nulls":7},{"v":125,"d":"Dn125"},"czujnik L=100mm",null,"osłona L=100mm",{"v":87.5,"d":"88"}]
[null,100,"xx","Dn100",{"$nulls":7},{"v":150,"d":"Dn150"},"czujnik L=100mm",null,"osłona L=100mm",100]
[null,"LC",{"v":1.5,"d":"Qn= 1.5 m3/h"},"Dn20",{"$nulls":7},{"v":200,"d":"Dn200"},"czujnik L=140mm",null,"osłona L=200mm",125]
[{"$nulls":11},{"v":250,"d":"Dn250"},"czujnik L=160mm",null,"osłona L=200mm",150]
[null,"Js","wodomierz jednostrumieniowy "]
[null,"Qn obl","Qn","Q3","Dn15"]
[null,0,1,1.6,"Dn15",{"$nulls":5},"WP",{"v":40,"d":"Dn40"},"czujnik L=45mm"]
[null,1,1.5,2.5,"Dn15",{"$nulls":5},"NP",{"v":40,"d":"Dn40"},0]
[null,1.5,2.5,4,"Dn20"]
[null,2.5,3.5,6.3,"Dn25"]
[null,3.5,6,10,"Dn32"]
[null,6,10,16,"Dn40"]
[null,10,15,25,"Dn50"]
[null,15]
[]
[null,"Js",{"v":1,"d":"Qn= 1.0 m3/h"},{"v":1.6,"d":"Q3= 1.6 m3/h"},"Dn15"]
{"$rows_empty":16}
[{"$nulls":3},"No-0131",null,null,"Wita Stwosza 1 ","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0132",null,null,"Wita Stwosza 2","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0133",null,null,"Wita Stwosza 4 ","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[null,null,"co+cw","No-0134",null,null,"Wita Stwosza 10","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0135",null,null,"Drużbackiej 1-3","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[null,null,"co+cw","No-0136",null,null,"Narutowicza 7","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0137",null,null,"Narutowicza 15","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0138",null,null,"Narutowicza 20","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0139",null,null,"Wita Stwosza 6","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek w trakcie sprzedaży",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0140",null,null,"Narutowicza 6 nowy","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek biurowy [nowy]",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0141",null,null,"Narutowicza 6 stary","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek biurowy [stary]",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0142",null,null,"Narutowicza 6 b-m","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek biurowo- magazynowy",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[null,null,"co wiszący","No-0143",null,null,"Narutowicza 9/2","negat TZP, brak zlecenia","OK",null,"Budynek mieszkalny wielorodzinny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0144",null,null,"Krakowska 40","oczekiwanie na wbór pomieszczenia","brak decyzji TZP",null,"Budynek mieszkalny wielorodzinny",{"$nulls":3},"TZP/5.1.1./130/05/2013",2014]
[{"$nulls":3},"No-0145",null,null,"Krakowska 42","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./130/05/2013",2014]
[null,null,"co wiszący","No-0146",null,null,"Narutowicza 7A-1, 7A-2","negat TZP, brak zlecenia","OK",null,"Budynek mieszkalny dwurodzinny",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[null,null,"co+cw","No-0147",null,null,"Krakowska 32","ZEST + RYS + AKPiA w TWR","OK",null,"Przychodnia ZOZ MSWIA",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[{"$nulls":3},"No-0148",null,null,"Bandrowskiego 4","ZEST + RYS + AKPiA w TWR","OK",null,"Zespół Szkół Nr 6",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[null,null,"co10m+60+cw30","No-0149",null,null,"Klikowska 31 Pyrek","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek handlowo- usługowy",{"$nulls":3},"TZP/5.1.1./147/05/2013","ok"]
[null,null,"co10 wiszący","No-0150",null,null,"Parkowa 20_1","w trakcie opracowania","jest umowa",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./147/05/2013","brak zgód raczej nie"]
[null,null,"b15_5","No-0151",null,null,"Skargi 38","w trakcie opracowania","jest umowa",null,"Budynek handlowo- usługowy",{"$nulls":3},"TZP/5.1.1./147/05/2013","brak zezw "]
[null,null,"co10 wiszący","No-0152",null,null,"Letnia 9","negat TZP, brak zlecenia","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","ok"]
[null,null,"co40 wiszący","No-0153",null,null,"Słoneczna 32","brak zlecenia","brak zezwoleń",null,"CenterMed poziom 1",{"$nulls":3},"TZP/5.1.1./150/05/2013","bank brak umowy"]
[null,null,"co80+cw60","No-0154",null,null,"Zielone 29 wz_1","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","ok"]
[null,null,"co105+cw60","No-0155",null,null,"Zielone 29 wz_2","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","ok"]
[null,null,"co30 wiszący","No-0156",null,null,"Widok 4","brak umowy, brak zlecenia","akt. brak umowy",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","w zawieszeniu brak umowy"]
[null,null,"co80","No-0157",null,null,"Sanguszków 20A","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","robimy"]
[null,null,"b30","No-0158",null,null,"Nowy Świat 16","ZEST + RYS + AKPiA w TWR","OK",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","awaria"]
[null,null,"co38 wiszący","No-0159",null,null,"Legionów 5A","negat TZP, brak zezwoleń, brak zlecenia","akt.?  brak umowy",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./150/05/2013","brak zezwoleni sieco"]
[null,null,"co+cw","No-0160",null,null,"Skargi 37","brak umowy, brak zlecenia","brak umowy",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./161/05/2013","brak zezwoleni sieco"]
[null,null,"??","No-0161",null,null,"??","??","??",null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./161/05/2013","brak zezwoleni sieco"]
[null,null,"co+cw wiszący","No-0162",null,null,"Węzeł wiszący CO wersja A i B","wycena + decyzja",null,null,"Budynek mieszkalny",{"$nulls":3},"TZP/5.1.1./161/05/2013","brak zezwoleni sieco"]
[null,null,"co??","No-0163",null,null,"Tarnovia węzeł + przepompownia","brak umowy, brak zlecenia","brak zlecenia",null,"nie bedzie"]
[null,null,"co?? wiszący","No-0164",null,null,"Tarnovia siłownia","brak umowy, brak zlecenia","brak zlecenia",null,"nie bedzie"]
[null,null,"co?? wiszący","No-0165",null,null,"Tarnovia biuro","brak umowy, brak zlecenia","brak zlecenia",null,"nie bedzie"]
[null,null,"co","No-0166",null,null,"Kochanowskiego 30 Intech",null,"OK",null,"Przychodnia ZOZ MSWIA",{"$nulls":3},"TZP/5.1.1./130/05/2013","ok"]
[]
[{"$nulls":3},"xxx","XXXXXXX",null,"Słowackiego 3 Dom Ogrodnika",{"$nulls":3},"rozmowy trwają"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Konarskiego 2 B",{"$nulls":3},"nie bedzie"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Szpital budynek L Szpitalna 13",{"$nulls":3},"nie bedzie"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Szpital budynek E Szpitalna 13",{"$nulls":3},"nie bedzie"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Wita Stwosza 9 Zaxon",{"$nulls":3},"nie bedzie"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Lwowska 43",{"$nulls":3},"nie bedzie"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Warzywna AWIM",{"$nulls":3},"nie bedzie"]
[{"$nulls":3},"xxx","XXXXXXX",null,"Kolejowa 33",{"$nulls":3},"nie bedzie"]
[]
[]
[{"$nulls":6},"Bardrowskiego szkoła + mieszkanie"]